**LED Display Receiving card HD-R501**

 **For Sending card HD-A601/602/603/HD-A30/A30+ series**

**Parameter：**



|  |  |
| --- | --- |
| **Type** | Indoor & outdoor full-color & single/dual color module |
| Scan mode | Static, 1-32 scan randomly |
| 1pcs of receiving card support areas | 256W\*192H(suggest).largest ：1024W×192H (single-dual color) |
| Receiving cards connected ways  | Receiving card set sequence randomly, it could recognize by automatically or by hand  |
| Gray scale | 0-65536 |
| Smart set | Smart set by few simple steps, through display routine setting ,it could suit almost different PCB routine  |
| Play contents | Play video、animation、picture、text、excel、PPT、time、counter etc |
| Test functions | It have self test button, could test modes of red、green、blue、white、gray、oblique line、grid、spots etc |
| Time on/time off | Time on /off display by defined and time on/off display by computer |
| Port | 2pin 5V Power x1,1000M Ethernet portX2，75B HUB portx12 |
| Voltage | 3V-6V |
| Working temperature |

|  |
| --- |
| -30℃-85℃ |

 |